FT-950 MENU SETTINGS
DATE:
MENU	DESCRIPTION 	SSB	SSB 60M	PSK31
  60M  
1.5KC 	 CW	   AM	FM	
1	AGC FAST TC	300		X	X			
2	AGC MID TC	700						
3	AGC SLOW TC	3000	X			X		
4	DISP COLOR DMU ONLY	-						
5	DISP FT950 DIM	5						
6	DISP BAR SEL (ZERO BEAT INDICATOR)	C-tn						
7	DISP PK HOLD S MTR	2						
8	DISP PK HOLD PWR OUT	2						
9	DISP PK HOLD ALC	2						
10	DISP PK DRAIN CURRENT	2						
11	DISP ROTOR START	-						
12	DISP ROTOR ADJ	-						
13	QMB DMU ONLY	-						
14	DVW RECORDER ONLY	-						
15	DVS RECORDER ONLY	-						
16	ENA BEACON	OFF						
17	NUMBER/SHORT CW	1290						
18	CONTEST # SET	1						
19	CW MEM 1 MODE	Typ 2						
20	CW MEM 2 MODE	Typ 2						
21	CW MEM 3 MODE	Typ 2						
22	CW MEM 4 MODE	Typ 2						
23	CW MEM 5 MODE	Typ 2						
24	ANT SELECT 1 - 2	2 - HF
1 - 6M						
25	BEEP LEVEL	50						
26	CAT BAUD RATE	4800						
27	CAT RTS TIMEOUT	3000						
28	CAT RTS ENABLE	ON						
29	MEM GROUP ON/OFF	OFF						
30	QUICK SPLIT VALUE	5						
31	TX TIMEOUT VALUE	OFF						
32	Utune COARSE/FINE	Stp 1						
33	MIC SCAN ENA	ON						
34	SCAN RESUME MODE	CAr						
35	FREQ DIAL CALIBRATE
!!!!DO NOT ADJUST!!!!	0						
36	AM MIKE GAIN FIX	35				35		
37	FRONT KEY MODE	ELE						
38	FRONT KEY NOR/REV	nor						
39	REAR KEY MODE	OFF						
40	REAR KEY NOR/REV	nor						
41	CW OK IN SSB MODE	On	OFF	OFF	ON	-		
42	CW CAR INJ USB/LSB
!!!!60 METERS!!!!	USB	USB	USB	USB	 - 		
43	CW FULL SEMI BK IN	1000						
44	CW SEMI TIME CONST 	1000						
45	CW PITCH FQ
!!!60 METERS !!!	700	700	700	700	-		
46	CW DOT-DASH RATIO	3,0						
47	CW FQ DISP OFFSET
!!! 60 METERS !!!	Ofst						
48	CW FROM RTTY JACK	dis						
49	DLY KEY TO RF OUT
PROTECTS AMP ARCS	30						
50	TNC LEVEL AFSK DATA	50						
51	AFSK LEVEL OUT DATA	50						
52	DATA VOX DELAY	300						
53	DATA VOX GAIN	50						
54	DATA PKT DISP OFFSET
!!! 60 METERS !!!	0						
55	DATA PKT CAR OFFSET
!!! 60 METERS !!!	0						
56	FM MIKE GAIN	50						
57	FM 10M RPT OFFSET	100						
58	FM 6M RPT OFFSET	1000						
59	RTTY RX POLARITY	nor						
60	RTTY TX POLARITY	nor						
61	RTTY OUT LEVEL	50						
62	RTTY SHIFT FREQ	170						
63	RTTY MARK TONE FQ	2125						
64	TX BANDWIDTH
!!! 60 METERS !!!	2 to 28	4 to 26	4 to 26	 - 	1 to 30		
65	LSB CARRIER FQ	0	0	0	0	0		
66	USB CARRIER FQ	0	0	0	0	0		
67	N BLANK SHORT LEVEL	220						
68	N BLANK LONG LEVEL	220						
69	CONTOUR FILT GAIN
SET FQ TO 700 FOR CW	20			ON*			
70	CONTOUR FILT Q	11						
71	DSP NOTCH ENA				OFF*	Maybe		
72	DIG NOISE FIL ENA/LVL	OFF						
73	SCOPE	-						
74	SCOPE	-						
75	SCOPE	-						
76	SCOPE	-						
77	SCOPE	-						
78	SCOPE	-						
79	SCOPE	-						
80	SCOPE	-						
81	SCOPE	-						
82	SCOPE	-						
83	SCOPE	-						
84	MAIN DIAL STEP SIZE	5						
85	CW 1 HZ STEP SIZE	ENA						
86	MHZ STEP SIZE	0,1						
87	UP/DN AM STEP	2,5						
88	UP/DN FM STEP	5						
89	FM DIAL TUN STEP
90 MYBAND NOT USED	100						
91	TX AUD EQ1 FQ	200		OFF				
92	TX AUD EQ1 GAIN	-12		OFF				
93	TX AUD EQ1 Q	1		OFF				
94	TX AUD EQ2 FQ	1500		OFF				
95	TX AUD EQ2 GAIN	-2		OFF				
96	TX AUD EQ2 Q	1		OFF				
97	TX AUD EQ3 FQ	2400		OFF				
98	TX AUD EQ3 GAIN	10		OFF				
99	TX AUD EQ3 Q	1		OFF				
100	TX AUD PROC EQ1 FQ	200		OFF				
101	TX AUD PROC EQ1 GAIN	-12		OFF				
102	TX AUD PROC EQ1 Q	1		OFF				
103	TX AUD PROC EQ2 FQ	1500		OFF				
104	TX AUD PROC EQ2 GAIN	-2		OFF				
105	TX AUD PROC EQ2 Q	1		OFF				
106	TX AUD PROC EQ3 FQ	2400		OFF				
107	TX AUD PROC EQ3 GAIN	10		OFF				
108	TX AUD PROC EQ3 Q	1		OFF				
109	TX AUD PROC LEVEL
ADJ IN AM OPTIMUM	23		OFF				
110	INT/EXT TUNER SEL	itu						
111	TX PWR LEVEL
SSB 100 FM 25 PSK 25	100	100	25	100	FIX
#112		
112	TX AM CARRIER LVL
20 WATTS BEST	-	-	-	-	35		
113	PWR CONTROL ALL	ALL						
114	TX VOX MIC/DATA SEL	data						
115	TX VOX VOICE LVL	50						
116	TX VOX VOICE DLY	500						
117	TX ANITVOX GAIN	0						
118	5.167.5 ENABLE	dis						
TX MTR MODE& *TUNR			ALC	ALC	SWR	ALC		
MONI	ON FOR CW	OFF	OFF	OPT	ON	OFF		
PROC	OFF FOR PACKET	ON	ON	OFF	-	ON		
BKIN KEYR		BKIN
KEYR	NO	NO	BKIN
KEYR			
AGC	AUTO WORKS OK	SLOW	SLOW	SLOW	FAST	SLOW		
*RX BW &
*CONT-OUR & *ROOF  FILTR		OPT

NO

3KC	OPT

NO

3KC	MAX 

NO

3KC	1.8 KC

YES

3KC	MAXBW

NO

6KC		
ITEMS WITH * ARE INCLUDED IN EACH FREQUENCY MEMORY

AM HAS OPTIMIZED SETTINGS FOR FIXED MIC GAIN, COMPRESSION
MAXIMUM TX BANDWIDTH

SSB HAS OPTIMIZED SETTINGS FOR TX BANDWIDTH, ESPECIALLY ON 60 METERS

CW AUDIO FREQUENCY IS 700, DONT CHANGE BECAUSE OF 60 METERS

FM IS 20 WATTS NO MORE, FIXED MIC GAIN, NO COMPRESSION 

PSK31 IS 20 WATTS NO MORE, MINIMUM TX BANDWIDTH, 1500 CENTER FOR 60 METERS

FOR 60 METERS, USE DIAL LOCK BUTTON ON MAIN TUNING WORK FROM MEMORY ONLY